**Human Performance Recognition**

**Needs Statement:**

Traditionally, live military exercises involving operations in urban terrain have relied heavily on the use of multiple instructor observers moving behind, beside, or above small units in training. Modernized live fire training ranges have undergone extensive instrumentation including Closed Circuit Television and long range night vision camera systems to provide safer and more thorough observation. While camera technology has increased in resolution and affordability, the reliance on instructor observers (human) processing multiple camera feeds into a single After Action Review (AAR) capability continues to be time consuming, and inconsistent (relying on individual instructor experience/knowledge).

With an increasing concern on affordability of range operations and cost to maintain infrastructure, a need has risen to evaluate the potential value of utilizing machine learning to automatically (and more consistently) identify human performance. Initial studies have already been made into the use of video analytics which to date have not satisfied all the operational requirements. As a result, an investigation has been requested into the use of human tracking and individual biometric sensor technologies which may provide individual and small unit level data streams, processed in real time by trained ML models.

The anticipated result would be reliable recognition of basic human activity (include positional movement and biometric recordings if possible). There is also uncertainty regarding the relative effect of variance in the sensor characteristics. Therefore, it is anticipated that the study will either evaluate, or account for the use of different sensor technologies. A conclusion should be made as to which sensor technologies provide the best recognition of human activity, using the same trained model.

Results shall be visualized in a way that provides a graphic representation of human activity based on different data sets and sensors, including the resultant classification of activity made by the trained model. Results shall include a distribution or categorization of at least two types of human subjects which compares an attribute of their performance (i.e. speed, endurance). This may require measurement of comparative heart rate to run rate, or distance over time, where the data supports the analysis.

Based on reliable data sets, provide a simulation of one or more soldiers (of different types), performing a specific drill or exercise, and demonstrate how accurately the trained model recognizes the human activity, and if possible, compare the relative performance of the soldiers.

**Approach:**

Select one or more of the following UCI datasets to train human activity recognition models. Compare the performance of the trained models on a normalized data set that utilizes the most essential attributes for basic activity recognition. Make observations regarding the techniques used to train the models, and identify the key parameters modified to achieve the most optimum result. Try to identify any factors in the data or techniques that constrain the performance of the model in successfully recognizing human activity. Which activities are the easiest to recognize, and which activities are the most difficult. Consider what aspects of the sensors (characteristics, number, location) might be the most important factors for successful recognition.

Analyze the normalized data set to determine the expected range of individual human performances. Select at least two types or categories of human activity and attempt to train the model to recognize the difference in performance (i.e. fast/slow run).

Build a mock scenario of two or more participants of different type / category, and visually demonstrate the use of the Human Performance Recognition capability. Document any observations and challenges made during the final demonstration. Build a flask based API that publishes two or more sensor data streams to the model, and provide a visual representation of the human activity with recognition results in real time.

**UCI Datasets:**

**Set 1:**

[https://archive.ics.uci.edu/ml/datasets/human+activity+recognition+using+smartphones#](https://archive.ics.uci.edu/ml/datasets/human+activity+recognition+using+smartphones)

|  |  |
| --- | --- |
| **Abstract**: Human Activity Recognition database built from the recordings of 30 subjects performing activities of daily living (ADL) while carrying a waist-mounted smartphone with embedded inertial sensors. |  |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Data Set Characteristics:** | Multivariate, Time-Series | **Number of Instances:** | 10299 | **Area:** | Computer |
| **Attribute Characteristics:** | N/A | **Number of Attributes:** | 561 | **Date Donated** | 2012-12-10 |
| **Associated Tasks:** | Classification, Clustering | **Missing Values?** | N/A | **Number of Web Hits:** | 841973 |

**Source:**

Jorge L. Reyes-Ortiz(1,2), Davide Anguita(1), Alessandro Ghio(1), Luca Oneto(1) and Xavier Parra(2)  
1 - Smartlab - Non-Linear Complex Systems Laboratory  
DITEN - Università degli Studi di Genova, Genoa (I-16145), Italy.   
2 - CETpD - Technical Research Centre for Dependency Care and Autonomous Living  
Universitat Politècnica de Catalunya (BarcelonaTech). Vilanova i la Geltrú (08800), Spain  
activityrecognition '@' smartlab.ws

**Data Set Information:**

The experiments have been carried out with a group of 30 volunteers within an age bracket of 19-48 years. Each person performed six activities (WALKING, WALKING\_UPSTAIRS, WALKING\_DOWNSTAIRS, SITTING, STANDING, LAYING) wearing a smartphone (Samsung Galaxy S II) on the waist. Using its embedded accelerometer and gyroscope, we captured 3-axial linear acceleration and 3-axial angular velocity at a constant rate of 50Hz. The experiments have been video-recorded to label the data manually. The obtained dataset has been randomly partitioned into two sets, where 70% of the volunteers was selected for generating the training data and 30% the test data.   
  
The sensor signals (accelerometer and gyroscope) were pre-processed by applying noise filters and then sampled in fixed-width sliding windows of 2.56 sec and 50% overlap (128 readings/window). The sensor acceleration signal, which has gravitational and body motion components, was separated using a Butterworth low-pass filter into body acceleration and gravity. The gravitational force is assumed to have only low frequency components, therefore a filter with 0.3 Hz cutoff frequency was used. From each window, a vector of features was obtained by calculating variables from the time and frequency domain.  
  
Check the README.txt file for further details about this dataset.   
  
A video of the experiment including an example of the 6 recorded activities with one of the participants can be seen in the following link: [[Web Link]](http://www.youtube.com/watch?v=XOEN9W05_4A)  
  
An updated version of this dataset can be found at [[Web Link]](http://archive.ics.uci.edu/ml/datasets/Smartphone-Based+Recognition+of+Human+Activities+and+Postural+Transitions). It includes labels of postural transitions between activities and also the full raw inertial signals instead of the ones pre-processed into windows.

**Attribute Information:**

For each record in the dataset it is provided:   
- Triaxial acceleration from the accelerometer (total acceleration) and the estimated body acceleration.   
- Triaxial Angular velocity from the gyroscope.   
- A 561-feature vector with time and frequency domain variables.   
- Its activity label.   
- An identifier of the subject who carried out the experiment.

**Relevant Papers:**

Davide Anguita, Alessandro Ghio, Luca Oneto, Xavier Parra and Jorge L. Reyes-Ortiz. Human Activity Recognition on Smartphones using a Multiclass Hardware-Friendly Support Vector Machine. International Workshop of Ambient Assisted Living (IWAAL 2012). Vitoria-Gasteiz, Spain. Dec 2012   
  
Davide Anguita, Alessandro Ghio, Luca Oneto, Xavier Parra, Jorge L. Reyes-Ortiz. Energy Efficient Smartphone-Based Activity Recognition using Fixed-Point Arithmetic. Journal of Universal Computer Science. Special Issue in Ambient Assisted Living: Home Care. Volume 19, Issue 9. May 2013  
  
Davide Anguita, Alessandro Ghio, Luca Oneto, Xavier Parra and Jorge L. Reyes-Ortiz. Human Activity Recognition on Smartphones using a Multiclass Hardware-Friendly Support Vector Machine. 4th International Workshop of Ambient Assited Living, IWAAL 2012, Vitoria-Gasteiz, Spain, December 3-5, 2012. Proceedings. Lecture Notes in Computer Science 2012, pp 216-223.   
  
Jorge Luis Reyes-Ortiz, Alessandro Ghio, Xavier Parra-Llanas, Davide Anguita, Joan Cabestany, Andreu Català. Human Activity and Motion Disorder Recognition: Towards Smarter Interactive Cognitive Environments. 21th European Symposium on Artificial Neural Networks, Computational Intelligence and Machine Learning, ESANN 2013. Bruges, Belgium 24-26 April 2013.

**Citation Request:**

Davide Anguita, Alessandro Ghio, Luca Oneto, Xavier Parra and Jorge L. Reyes-Ortiz. A Public Domain Dataset for Human Activity Recognition Using Smartphones. 21th European Symposium on Artificial Neural Networks, Computational Intelligence and Machine Learning, ESANN 2013. Bruges, Belgium 24-26 April 2013.

Set 2:

<https://archive.ics.uci.edu/ml/datasets/Localization+Data+for+Person+Activity>

|  |  |
| --- | --- |
| **Abstract**: Data contains recordings of five people performing different activities. Each person wore four sensors (tags) while performing the same scenario five times. |  |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Data Set Characteristics:** | Univariate, Sequential, Time-Series | **Number of Instances:** | 164860 | **Area:** | Life |
| **Attribute Characteristics:** | Real | **Number of Attributes:** | 8 | **Date Donated** | 2010-11-03 |
| **Associated Tasks:** | Classification | **Missing Values?** | N/A | **Number of Web Hits:** | 95504 |

**Source:**

- Creators: Mitja Lustrek (mitja.lustrek **'@'** ijs.si), Bostjan Kaluza (bostjan.kaluza **'@'** ijs.si), Rok Piltaver (rok.piltaver **'@'** ijs.si), Jana Krivec (jana.krivec **'@'** ijs.si), Vedrana Vidulin (vedrana.vidulin **'@'** ijs.si)   
- Jozef Stefan Institute, Jamova cesta 39, 1000 Ljubljana, Slovenija   
- Donor: Bozidara Cvetkovic (boza.cvetkovic **'@'** ijs.si)   
- Jozef Stefan Institute, Jamova cesta 39, 1000 Ljubljana, Slovenija   
- Date received: October, 2010

**Data Set Information:**

People used for recording of the data were wearing four tags (ankle left, ankle right, belt and chest).   
Each instance is a localization data for one of the tags. The tag can be identified by one of the attributes.

1) Sequence Name {A01,A02,A03,A04,A05,B01,B02,B03,B04,B05,C01,C02,C03,C04,C05,D01,D02,D03,D04,D05,E01,E02,E03,E04,E05} (Nominal)   
- A, B, C, D, E = 5 people   
2) Tag identificator {010-000-024-033,020-000-033-111,020-000-032-221,010-000-030-096} (Nominal)   
- ANKLE\_LEFT = 010-000-024-033   
- ANKLE\_RIGHT = 010-000-030-096   
- CHEST = 020-000-033-111   
- BELT = 020-000-032-221   
3) timestamp (Numeric) all unique   
4) date FORMAT = dd.MM.yyyy HH:mm:ss:SSS (Date)   
5) x coordinate of the tag (Numeric)   
6) y coordinate of the tag (Numeric)   
7) z coordinate of the tag (Numeric)   
8) activity {walking,falling,'lying down',lying,'sitting down',sitting,'standing up from lying','on all fours','sitting on the ground','standing up from sitting','standing up from sitting on the ground'} (Nominal)

**Relevant Papers:**

B. Kaluza, V. Mirchevska, E. Dovgan, M. Lustrek, M. Gams, An Agent-based Approach to Care in Independent Living, International Joint Conference on Ambient Intelligence (AmI-10), Malaga, Spain, In press

**Citation Request:**

B. Kaluza, V. Mirchevska, E. Dovgan, M. Lustrek, M. Gams, An Agent-based Approach to Care in Independent Living, International Joint Conference on Ambient Intelligence (AmI-10), Malaga, Spain, In press

Set 3:

<http://archive.ics.uci.edu/ml/datasets/pamap2+physical+activity+monitoring>

|  |  |
| --- | --- |
| **Abstract**: The PAMAP2 Physical Activity Monitoring dataset contains data of 18 different physical activities, performed by 9 subjects wearing 3 inertial measurement units and a heart rate monitor. |  |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Data Set Characteristics:** | Multivariate, Time-Series | **Number of Instances:** | 3850505 | **Area:** | Computer |
| **Attribute Characteristics:** | Real | **Number of Attributes:** | 52 | **Date Donated** | 2012-08-06 |
| **Associated Tasks:** | Classification | **Missing Values?** | Yes | **Number of Web Hits:** | 78253 |

**Source:**

Attila Reiss, Department Augmented Vision, DFKI, Germany, attila.reiss '@' dfki.de   
Date: August 2012.

**Data Set Information:**

The PAMAP2 Physical Activity Monitoring dataset contains data of 18 different physical activities (such as walking, cycling, playing soccer, etc.), performed by 9 subjects wearing 3 inertial measurement units and a heart rate monitor. The dataset can be used for activity recognition and intensity estimation, while developing and applying algorithms of data processing, segmentation, feature extraction and classification.   
  
\*\* Sensors \*\*   
3 Colibri wireless inertial measurement units (IMU):   
- sampling frequency: 100Hz   
- position of the sensors:   
- 1 IMU over the wrist on the dominant arm   
- 1 IMU on the chest   
- 1 IMU on the dominant side's ankle   
HR-monitor:   
- sampling frequency: ~9Hz   
  
\*\* Data collection protocol \*\*   
Each of the subjects had to follow a protocol, containing 12 different activities. The folder â€œProtocolâ€ contains these recordings by subject.   
Furthermore, some of the subjects also performed a few optional activities. The folder â€œOptionalâ€ contains these recordings by subject.   
  
\*\* Data files \*\*   
Raw sensory data can be found in space-separated text-files (.dat), 1 data file per subject per session (protocol or optional). Missing values are indicated with NaN. One line in the data files correspond to one timestamped and labeled instance of sensory data. The data files contain 54 columns: each line consists of a timestamp, an activity label (the ground truth) and 52 attributes of raw sensory data.

**Attribute Information:**

The 54 columns in the data files are organized as follows:   
1. timestamp (s)   
2. activityID (see below for the mapping to the activities)   
3. heart rate (bpm)   
4-20. IMU hand   
21-37. IMU chest   
38-54. IMU ankle   
  
The IMU sensory data contains the following columns:   
1. temperature (Â°C)   
2-4. 3D-acceleration data (ms-2), scale: Â±16g, resolution: 13-bit   
5-7. 3D-acceleration data (ms-2), scale: Â±6g, resolution: 13-bit   
8-10. 3D-gyroscope data (rad/s)   
11-13. 3D-magnetometer data (Î¼T)   
14-17. orientation (invalid in this data collection)   
  
List of activityIDs and corresponding activities:   
1 lying   
2 sitting   
3 standing   
4 walking   
5 running   
6 cycling   
7 Nordic walking   
9 watching TV   
10 computer work   
11 car driving   
12 ascending stairs   
13 descending stairs   
16 vacuum cleaning   
17 ironing   
18 folding laundry   
19 house cleaning   
20 playing soccer   
24 rope jumping   
0 other (transient activities)

**Relevant Papers:**

The following two publications describe the dataset and provide a baseline benchmark on various tasks of physical activity recognition and intensity estimation:   
  
[1] A. Reiss and D. Stricker. Introducing a New Benchmarked Dataset for Activity Monitoring. The 16th IEEE International Symposium on Wearable Computers (ISWC), 2012.   
[2] A. Reiss and D. Stricker. Creating and Benchmarking a New Dataset for Physical Activity Monitoring. The 5th Workshop on Affect and Behaviour Related Assistance (ABRA), 2012.   
  
Further information (detailed description of the protocol and the various activities, statistics of the dataset, the subjects, etc.) can be found in the documentation attached to the dataset. Please refer to the file readme.pdf.

**Citation Request:**

This dataset is freely available for academic research, there are no (legal or other) constraints on using the data for scientific purposes. We would appreciate referencing one of the below publications ([1] or [2]) if you use this dataset.   
If you have any questions or suggestions, please contact Attila Reiss ([firstname].[lastname]@dfki.de). Also, please let us know if you have any publications that uses this dataset.   
We recommend to refer to this dataset as the â€œPAMAP2 Datasetâ€ or the â€œPAMAP2 Physical Activity Monitoring Datasetâ€.   
  
[1] A. Reiss and D. Stricker. Introducing a New Benchmarked Dataset for Activity Monitoring. The 16th IEEE International Symposium on Wearable Computers (ISWC), 2012.   
[2] A. Reiss and D. Stricker. Creating and Benchmarking a New Dataset for Physical Activity Monitoring. The 5th Workshop on Affect and Behaviour Related Assistance (ABRA), 2012.

Set 4:

<https://archive.ics.uci.edu/ml/datasets/Activities+of+Daily+Living+%28ADLs%29+Recognition+Using+Binary+Sensors>

|  |  |
| --- | --- |
| **Abstract**: This dataset comprises information regarding the ADLs performed by two users on a daily basis in their own homes. |  |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Data Set Characteristics:** | Multivariate, Sequential, Time-Series | **Number of Instances:** | 2747 | **Area:** | Computer |
| **Attribute Characteristics:** | N/A | **Number of Attributes:** | N/A | **Date Donated** | 2013-10-28 |
| **Associated Tasks:** | Classification, Clustering | **Missing Values?** | N/A | **Number of Web Hits:** | 81169 |

**Source:**

Francisco Javier OrdÃ³Ã±ez, Carlos III University of Madrid, fordonez **'@'** inf.uc3m.es

**Data Set Information:**

This dataset comprises information regarding the ADLs performed by two users on a daily basis in their   
own homes. This dataset is composed by two instances of data, each one corresponding to a different   
user and summing up to 35 days of fully labelled data. Each instance of the dataset is described by   
three text files, namely: description, sensors events (features), activities of the daily living (labels).   
Sensor events were recorded using a wireless sensor network and data were labelled manually.

**Attribute Information:**

The features are the sensor events captured for the corresponding Wireless Sensor Network.

**Relevant Papers:**

N/A

**Citation Request:**

OrdÃ³Ã±ez, F.J.; de Toledo, P.; Sanchis, A. Activity Recognition Using Hybrid Generative/Discriminative Models on Home Environments Using Binary Sensors. Sensors 2013, 13, 5460-5477.

Set 6:

<https://archive.ics.uci.edu/ml/datasets/Activity+Recognition+system+based+on+Multisensor+data+fusion+(AReM)>

|  |  |
| --- | --- |
| **Abstract**: This dataset contains temporal data from a Wireless Sensor Network worn by an actor performing the activities: bending, cycling, lying down, sitting, standing, walking. |  |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Data Set Characteristics:** | Multivariate, Sequential, Time-Series | **Number of Instances:** | 42240 | **Area:** | Computer |
| **Attribute Characteristics:** | Real | **Number of Attributes:** | 6 | **Date Donated** | 2016-05-18 |
| **Associated Tasks:** | Classification | **Missing Values?** | N/A | **Number of Web Hits:** | 48693 |

**Source:**

Filippo Palumbo (a,b), Claudio Gallicchio (b), Rita Pucci (b) and Alessio Micheli (b)   
  
(a) Institute of Information Science and Technologies â€œAlessandro Faedoâ€, National Research Council, Pisa, Italy   
(b) Department of Computer Science, University of Pisa, Pisa, Italy

**Data Set Information:**

This dataset represents a real-life benchmark in the area of Activity Recognition applications, as described in [1].   
  
The classification tasks consist in predicting the activity performed by the user from time-series generated by a Wireless Sensor Network (WSN), according to the EvAAL competition technical annex ([[Web Link]](http://evaal.aaloa.org/)).   
  
In our activity recognition system we use information coming the implicit alteration of the wireless channel due to the movements of the user. The devices measure the RSS of the beacon packets they exchange among themselves in the WSN [2].   
  
We collect RSS data using IRIS nodes embedding a Chipcon AT86RF230 radio subsystem that implements the IEEE 802.15.4 standard and programmed with a TinyOS firmware. They are placed on the userâ€™s chest and ankles. For the purpose of communications, the beacon packets are exchanged by using a simple virtual token protocol that completes its execution in a time slot of 50 milliseconds. A modified version of the Spin ([[Web Link]](http://span.ece.utah.edu/spin)) token-passing protocol is used to schedule node transmission, in order to prevent packet collisions and maintain high data collection rate. When an anchor is transmitting, all other anchors receive the packet and perform the RSS measurements. The payload of the transmitting packet is the set of RSS values between the transmitting node and the other sensors sampled during the previous cycle.   
  
From the raw data we extract time-domain features to compress the time series and slightly remove noise and correlations.   
  
We choose an epoch time of 250 milliseconds according to the EVAAL technical annex. In such a time slot we elaborate 5 samples of RSS (sampled at 20 Hz) for each of the three couples of WSN nodes (i.e. Chest-Right Ankle, Chest-Left Ankle, Right Ankle-Left Ankle). The features include the mean value and standard deviation for each reciprocal RSS reading from worn WSN sensors.   
  
For each activity 15 temporal sequences of input RSS data are present. The dataset contains 480 sequences, for a total number of 42240 instances.   
  
We also consider two kind of bending activity, illustrated in the figure provided (bendingTupe.pdf). The positions of sensor nodes with the related identifiers are shown in figure sensorsPlacement.pdf.

**Attribute Information:**

For each sequence, data is provided in comma separated value (csv) format.   
  
- Input data:   
Input RSS streams are provided in files named datasetID.csv, where ID is the progressive numeric sequence ID for each repetition of the activity performed.   
In each file, each row corresponds to a time step measurement (in temporal order) and contains the following information:   
avg\_rss12, var\_rss12, avg\_rss13, var\_rss13, avg\_rss23, var\_rss23   
where avg and var are the mean and variance values over 250 ms of data, respectively.   
  
- Target data:   
Target data is provided as the containing folder name.   
  
For each activity, we have the following parameters:   
# Frequency (Hz): 20   
# Clock (millisecond): 250   
# Total duration (seconds): 120

**Relevant Papers:**

[1] F. Palumbo, C. Gallicchio, R. Pucci and A. Micheli, Human activity recognition using multisensor data fusion based on Reservoir Computing, Journal of Ambient Intelligence and Smart Environments, 2016, 8 (2), pp. 87-107.   
[2] F. Palumbo, P. Barsocchi, C. Gallicchio, S. Chessa and A. Micheli, Multisensor data fusion for activity recognition based on reservoir computing, in: Evaluating AAL Systems Through Competitive Benchmarking, Communications in Computer and Information Science, Vol. 386, Springer, Berlin, Heidelberg, 2013, pp. 24â€“35.

**Citation Request:**

F. Palumbo, C. Gallicchio, R. Pucci and A. Micheli, Human activity recognition using multisensor data fusion based on Reservoir Computing, Journal of Ambient Intelligence and Smart Environments, 2016, 8 (2), pp. 87-107.

Set 6:

<https://archive.ics.uci.edu/ml/datasets/UbiqLog+(smartphone+lifelogging)>

|  |  |
| --- | --- |
| **Abstract**: UbiqLog is the smartphone lifelogging tool that runs on the smartphone of 35 users for about 2 months. |  |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Data Set Characteristics:** | Multivariate | **Number of Instances:** | 9782222 | **Area:** | Computer |
| **Attribute Characteristics:** | N/A | **Number of Attributes:** | N/A | **Date Donated** | 2016-06-16 |
| **Associated Tasks:** | Causal-Discovery | **Missing Values?** | N/A | **Number of Web Hits:** | 24242 |

**Source:**

Reza Rawassizadeh rrawassizadeh **'@'** acm.org. University of California Riverside.

**Data Set Information:**

This is the first smartphone based lifelogging dataset that is going to be available for public use. Please consider that the user of this dataset are obliged NOT to perform any sort of analysis that can harm the privacy of participants. This dataset is not for any privacy related analysis that can re-identify users.   
The UbiqLog tool is open source and accessible here: [[Web Link]](https://github.com/Rezar/Ubiqlog)

**Attribute Information:**

With respect to users privacy UbiqLog collects their Calls, SMS headers (no content), App use, WiFi & Bluetooth devices in user's proximity, geographical location (if available and GPS works), physical activities form Google play API.   
Data format is in JSON, because there are different sensors and they have different variables. Nevertheless, we have the code for cleaning and converting the data into CSV + smoothing the time. Moreover, we can share our visualization code. Interested individuals could contact the given email address.

**Relevant Papers:**

To appear: Scalable Daily Human Behavioral Pattern Mining from Multivariate Temporal Data.

**Citation Request:**

Please cite both of the following paper and NOT only one of them:   
  
Rawassizadeh, R., Tomitsch, M., Wac, K., & Tjoa, A. M. (2013). UbiqLog: a generic mobile phone-based life-log framework. Personal and ubiquitous computing, 17(4), 621-637.   
  
Rawassizadeh, R., Momeni, E., Dobbins, C., Mirza-Babaei, P., & Rahnamoun, R. (2015). Lesson Learned from Collecting Quantified Self Information via Mobile and Wearable Devices. Journal of Sensor and Actuator Networks, 4(4), 315-335.

Set 7:

<https://archive.ics.uci.edu/ml/datasets/WESAD+%28Wearable+Stress+and+Affect+Detection%29>

|  |  |
| --- | --- |
| **Abstract**: WESAD (Wearable Stress and Affect Detection) contains data of 15 subjects during a stress-affect lab study, while wearing physiological and motion sensors. |  |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Data Set Characteristics:** | Multivariate, Time-Series | **Number of Instances:** | 63000000 | **Area:** | Computer |
| **Attribute Characteristics:** | Real | **Number of Attributes:** | 12 | **Date Donated** | 2018-09-14 |
| **Associated Tasks:** | Classification, Regression | **Missing Values?** | N/A | **Number of Web Hits:** | 16566 |

**Source:**

Philip Schmidt, Robert Bosch GmbH, Corporate Research, Germany, firstname.lastname **'@'** de.bosch.com   
Attila Reiss, Robert Bosch GmbH, Corporate Research, Germany, firstname.lastname **'@'** de.bosch.com

**Data Set Information:**

WESAD is a publicly available dataset for wearable stress and affect detection. This multimodal dataset features physiological and motion data, recorded from both a wrist- and a chest-worn device, of 15 subjects during a lab study. The following sensor modalities are included: blood volume pulse, electrocardiogram, electrodermal activity, electromyogram, respiration, body temperature, and three-axis acceleration. Moreover, the dataset bridges the gap between previous lab studies on stress and emotions, by containing three different affective states (neutral, stress, amusement). In addition, self-reports of the subjects, which were obtained using several established questionnaires, are contained in the dataset. Details can be found in the dataset's readme-file, as well as in [1].

**Attribute Information:**

Raw sensor data was recorded with two devices: a chest-worn device (RespiBAN) and a wrist-worn device (Empatica E4).   
The RespiBAN device provides the following sensor data: electrocardiogram (ECG), electrodermal activity (EDA), electromyogram (EMG), respiration, body temperature, and three-axis acceleration. All signals are sampled at 700 Hz.   
The Empatica E4 device provides the following sensor data: blood volume pulse (BVP, 64 Hz), electrodermal activity (EDA, 4 Hz), body temperature (4 Hz), and three-axis acceleration (32 Hz).   
  
The dataset's readme-file contains all further details with respect to the dataset structure, data format (RespiBAN device, Empatica E4 device, synchronised data), study protocol, and the self-report questionnaires.

**Relevant Papers:**

[1] Philip Schmidt, Attila Reiss, Robert Duerichen, Claus Marberger and Kristof Van Laerhoven. 2018. Introducing WESAD, a multimodal dataset for Wearable Stress and Affect Detection. In 2018 International Conference on Multimodal Interaction (ICMI â€™18), October 16â€“20, 2018, Boulder, CO, USA. ACM, New York, NY, USA, 9 pages. [[Web Link]](https://doi.org/10.1145/3242969.3242985)

**Citation Request:**

You may use this data for scientific, non-commercial purposes, provided that you give credit to the owners when publishing any work based on this data. Please acknowledge publication [1].   
We recommend to refer to this dataset as WESAD, or 'Wearable Stress and Affect Detection'.